; 
;  Purpose: Netcard setup information file for WFW311
;
;  Author:  Charles Yu
; 
;  Date:    Nov, 2003
; 
 
[data]
type=network
; VERSION.... 3.12
version=3.11.312

[disks]
; source disk
1=.,"VIA Rhine Family Fast Ethernet Adapter Driver Disk", fetnd3f.386

[netcard]
; OEM....
;   key = description, MSID, type, media, mode, install, protini, style
fet$3043="VIA VT86C100A Rhine Fast Ethernet Adapter",0,ndis,ethernet,0x07,fet$nd3f,fet$3043_nif
fet$3065="VIA Rhine II Fast Ethernet Adapter",0,ndis,ethernet,0x07,fet$nd3f,fet$3065_nif
fet$3106J="VIA Rhine III Fast Ethernet Adapter",0,ndis,ethernet,0x07,fet$nd3f,fet$3106J_nif
fet$3106S="VIA Rhine III Management Adapter",0,ndis,ethernet,0x07,fet$nd3f,fet$3106S_nif



[fet$nd3f]
ndis3=1:fetnd3f.386
ndis2=1:fetnd.dos
mlid=*:fetodi.com

[fet$3106J_nif]
; NDIS2 driver parameters:
drivername=FETND$,0x10
param=FULLDUPLEX,"[NDIS2] DUPLEX MODE",enum,"Half_Duplex,0,Full_Duplex,1",0,0x10
param=SPEED,"[NDIS2] SPEED MODE",enum,"10M,10,100M,100",100,0x10
param=AUTO,"[NDIS2] AUTO MODE",enum,"Auto-Negotiation,1,Force-Mode,0",1,0x10
param=SLOT,"[NDIS2] SLOT NUMBER",int,"1,16,1",1,0x10

; NDIS3 driver parameters:
param=AdapterCFID,"Adapter CFID",static,"822481158",,0x20
param=AdapterType,"Adapter Type",static,"5",,0x20
param=MediaType,"Media Type",static,"1",,0x20
param=BusType,"Bus Type",static,"5",,0x20
; WFW_311
param=OsId,"Os Id",static,"00000002",,0x20
param=ConnectionType,"[NDIS3] Connection Type",enum,"Auto-Negotiation,0,100BaseTx Half_Duplex,1,100BaseTx Full_Duplex,2, 10BaseT   Half_Duplex,3, 10BaseT Full_Duplex,4",0,0x20
; 
param=ReceiveBuffers,"Receive Buffers",static,"64",,0x20
param=TransmitBuffers,"Transmit Buffers",static,"32",,0x20
param=ReceiveThreshold,"Receive Threshold",static,"0",,0x20
param=TransmitThreshold,"Transmit Threshold",static,"0",,0x20
param=BurstLength,"Burst Length",static,"1",,0x20
param=MapRegisters,"Map Registers",static,"16",,0x20
param=EarlyReceive,"Early Receive",static,"0",,0x20
param=EarlyTransmit,"Early Transmit",static,"0",,0x20
param=NwayForce,"Nway Force",static,"1",,0x20
param=FlowCtrl,"[NDIS3] Flow Control",enum,"Hardware_Default,0,Disable,1,Enable,2",0,0x20
param=ValPktLen,"Validate Packet Length",static,"0",,0x20


[fet$3106S_nif]
; NDIS2 driver parameters:
drivername=FETND$,0x10
param=FULLDUPLEX,"[NDIS2] DUPLEX MODE",enum,"Half_Duplex,0,Full_Duplex,1",0,0x10
param=SPEED,"[NDIS2] SPEED MODE",enum,"10M,10,100M,100",100,0x10
param=AUTO,"[NDIS2] AUTO MODE",enum,"Auto-Negotiation,1,Force-Mode,0",1,0x10
param=SLOT,"[NDIS2] SLOT NUMBER",int,"1,16,1",1,0x10

; NDIS3 driver parameters:
param=AdapterCFID,"Adapter CFID",static,"810750214",,0x20
param=AdapterType,"Adapter Type",static,"5",,0x20
param=MediaType,"Media Type",static,"1",,0x20
param=BusType,"Bus Type",static,"5",,0x20
; WFW_311
param=OsId,"Os Id",static,"00000002",,0x20
param=ConnectionType,"[NDIS3] Connection Type",enum,"Auto-Negotiation,0,100BaseTx Half_Duplex,1,100BaseTx Full_Duplex,2, 10BaseT   Half_Duplex,3, 10BaseT Full_Duplex,4",0,0x20
; 
param=ReceiveBuffers,"Receive Buffers",static,"64",,0x20
param=TransmitBuffers,"Transmit Buffers",static,"32",,0x20
param=ReceiveThreshold,"Receive Threshold",static,"0",,0x20
param=TransmitThreshold,"Transmit Threshold",static,"0",,0x20
param=BurstLength,"Burst Length",static,"1",,0x20
param=MapRegisters,"Map Registers",static,"16",,0x20
param=EarlyReceive,"Early Receive",static,"0",,0x20
param=EarlyTransmit,"Early Transmit",static,"0",,0x20
param=NwayForce,"Nway Force",static,"1",,0x20
param=FlowCtrl,"[NDIS3] Flow Control",enum,"Hardware_Default,0,Disable,1,Enable,2",0,0x20
param=ValPktLen,"Validate Packet Length",static,"0",,0x20


[fet$3065_nif]
; NDIS2 driver parameters:
drivername=FETND$,0x10
param=FULLDUPLEX,"[NDIS2] DUPLEX MODE",enum,"Half_Duplex,0,Full_Duplex,1",0,0x10
param=SPEED,"[NDIS2] SPEED MODE",enum,"10M,10,100M,100",100,0x10
param=AUTO,"[NDIS2] AUTO MODE",enum,"Auto-Negotiation,1,Force-Mode,0",1,0x10
param=SLOT,"[NDIS2] SLOT NUMBER",int,"1,16,1",1,0x10

; NDIS3 driver parameters:
param=AdapterCFID,"Adapter CFID",static,"811929862",,0x20
param=AdapterType,"Adapter Type",static,"5",,0x20
param=MediaType,"Media Type",static,"1",,0x20
param=BusType,"Bus Type",static,"5",,0x20
; WFW_311
param=OsId,"Os Id",static,"00000002",,0x20
param=ConnectionType,"[NDIS3] Connection Type",enum,"Auto-Negotiation,0,100BaseTx Half_Duplex,1,100BaseTx Full_Duplex,2, 10BaseT   Half_Duplex,3, 10BaseT Full_Duplex,4",0,0x20
; 
param=ReceiveBuffers,"Receive Buffers",static,"64",,0x20
param=TransmitBuffers,"Transmit Buffers",static,"32",,0x20
param=ReceiveThreshold,"Receive Threshold",static,"0",,0x20
param=TransmitThreshold,"Transmit Threshold",static,"0",,0x20
param=BurstLength,"Burst Length",static,"1",,0x20
param=MapRegisters,"Map Registers",static,"16",,0x20
param=EarlyReceive,"Early Receive",static,"0",,0x20
param=EarlyTransmit,"Early Transmit",static,"0",,0x20
param=NwayForce,"Nway Force",static,"1",,0x20
param=FlowCtrl,"[NDIS3] Flow Control",enum,"Hardware_Default,0,Disable,1,Enable,2",0,0x20
param=ValPktLen,"Validate Packet Length",static,"0",,0x20


[fet$3043_nif]
; NDIS2 driver parameters:
drivername=FETND$,0x10
param=FULLDUPLEX,"[NDIS2] DUPLEX MODE",enum,"Half_Duplex,0,Full_Duplex,1",0,0x10
param=SPEED,"[NDIS2] SPEED MODE",enum,"10M,10,100M,100",100,0x10
param=AUTO,"[NDIS2] AUTO MODE",enum,"Auto-Negotiation,1,Force-Mode,0",1,0x10
param=SLOT,"[NDIS2] SLOT NUMBER",int,"1,16,1",1,0x10

; NDIS3 driver parameters:
param=AdapterCFID,"Adapter CFID",static,"809701638",,0x20
param=AdapterType,"Adapter Type",static,"5",,0x20
param=MediaType,"Media Type",static,"1",,0x20
param=BusType,"Bus Type",static,"5",,0x20
; WFW_311
param=OsId,"Os Id",static,"00000002",,0x20
param=ConnectionType,"[NDIS3] Connection Type",enum,"Auto-Negotiation,0,100BaseTx Half_Duplex,1,100BaseTx Full_Duplex,2, 10BaseT   Half_Duplex,3, 10BaseT   Full_Duplex,4",0,0x20
; 
param=ReceiveBuffers,"Receive Buffers",static,"64",,0x20
param=TransmitBuffers,"Transmit Buffers",static,"8",,0x20
param=ReceiveThreshold,"Receive Threshold",static,"0",,0x20
param=TransmitThreshold,"Transmit Threshold",static,"0",,0x20
param=BurstLength,"Burst Length",static,"1",,0x20
param=MapRegisters,"Adapter Type",static,"8",,0x20
param=EarlyReceive,"Early Receive",static,"0",,0x20
param=EarlyTransmit,"Adapter Type",static,"0",,0x20
param=ValPktLen,"Validate Packet Length",static,"0",,0x20
