;
;  Purpose:   Netcard setup information file for Windows 95(OSR2) / 98(SE) / ME / 2000 / XP
;
;  Author:    Tevin Chen
;
;  Date:      Nov, 2003
;
;  Copyright: VIA Technologies, Inc.
;

[Version]
CatalogFile = netvt.cat
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Prov%
DriverVer   = 11/11/2003,3.27.0.0412

[Manufacturer]
%Manuf%       = MANUF

[MANUF]
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_01061106
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_01051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01021106
%VT3043.DeviceDesc% = VT3043.ndi,   PCI\VEN_1106&DEV_3043&SUBSYS_01001106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065
%VT3043.DeviceDesc% = VT3043.ndi,   PCI\VEN_1106&DEV_3043

;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_02001014
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_029014CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_466014CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_466A14CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_800114CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_700114CD
;(8)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70681071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_71701071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_73681071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01241071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_85561071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_83751071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_102213BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_102413BD
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A70110FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A70010FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71510FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71610FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71710FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A80010FD
;(4)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81001584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81101584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81201584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10321734
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_15031043
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_80C71043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80C71043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80FF1043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80A11043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80ED1043
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_101E1025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_003E1025
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B710156D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B7261019
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_3185109F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7143109F
;(26)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90011509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_901F1509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90211509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90221509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90231509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90241509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90251509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90261509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90271509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90281509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_28201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90481509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92121509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_905F1509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92161509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_35301509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90561509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92211509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92321509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92331509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92341509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92351509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92361509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92571509
;(15)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0077A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0088A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00C3A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00C7A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_016FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_042FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_041DA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_042FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0439A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_046FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_044BA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_043AA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04CFA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04D1A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04D2A0A0
;(3)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70021631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_D0021631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_D0031631
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10291025
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0028103C
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0001458
;(6)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_900B1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_900B1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30031695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30051695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30041695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30061695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_217614A4
;(49)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A2321297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8001297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8011297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8021297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8031297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8041297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8051297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8061297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8071297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8081297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8091297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80F1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8101297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8111297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8121297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8131297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8141297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8151297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8161297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8171297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8181297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8191297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81F1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8201297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8211297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8221297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8231297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8241297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8251297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8261297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8271297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8281297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8291297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82F1297
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_15D40015
;(14)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_2718270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_2718270F
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_271B270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_271B270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7552270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7553270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7576270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7577270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7578270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7649270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7660270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7664270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7668270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7669270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7178270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7840270F
;(3)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1400147B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1401147B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1402147B
;(52)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A781019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A791019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A801019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A811019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A821019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A831019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A841019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A851019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A861019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18311019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18321019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18331019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18341019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18351019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18361019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18371019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18381019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18391019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18401019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18411019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18421019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18431019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18441019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18451019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18461019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18471019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18481019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18491019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18501019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18511019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18521019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18531019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18541019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18551019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18561019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18571019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18581019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18591019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18601019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A361019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A691019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A711019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A721019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A731019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A741019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A751019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A761019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A771019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F101019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B7261019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B3201019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F251019
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00011843
;(9)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10011816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10011816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10021816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10021816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10041816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10041816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10051816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10051816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_40011816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_40011816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_40021816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_40021816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_30011816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30011816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20021816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20011816
;(4)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5150107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5151107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5130107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5135107D
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_233310F1
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_249010F1
;(28)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60101106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60151106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60171106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0031106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0041106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0061106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0091106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_B0031106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_B0051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0061106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0021106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0031106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0051106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0061106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA011106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA021106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA031106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA041106
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_AA051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_CC011106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_CC021106
;(22)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_390C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_593C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_596C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_712C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_716C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_707C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_72301462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_723C1462
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_747C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_747C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_762C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_768C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_775C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_778C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_015C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_014C1462
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_012C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_012C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_750C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C01C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C02C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C03C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C04C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_021C1462
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_140217F2
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_140617F2
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_140617F2
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30431849
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_923017C4
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_8000105B
;(3)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_217514A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_217514A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_218214A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_217614A4
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_040814FF
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_202B161F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_2032161F
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_001214C0
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_200A1558
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00331025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0713152D
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00011170
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00021170
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_010216F3
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_010516F3
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_010516F3
;(16)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120018D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120118D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120218D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120318D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120418D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120518D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120618D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120718D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120818D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120918D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120A18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120B18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120C18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120D18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120E18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120F18D0
;-------------------------------------------------------------------------------
; ndi for 3106S
;-------------------------------------------------------------------------------
[VT3106S.ndi]
DelReg          = FET.delreg
AddReg          = VT3106S.reg, FET.reg, FlowCtrl.reg, FET.reg.win, AI.reg, Tagging.reg, VLAN.reg
CopyFiles       = FET.ndi.CopyFiles

[VT3106S.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg
AddReg          = VT3106S.reg, FET.reg, FlowCtrl.reg, FET.reg.NT, AI.reg, Tagging.reg, VLAN.reg, Cksumoffload.reg.NT
CopyFiles       = FET.CopyFiles.NT

[VT3106S.ndi.NT.Services]
AddService      = FETNDISB, 2, FET.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3106J
;-------------------------------------------------------------------------------
[VT3106J.ndi]
DelReg          = FET.delreg
AddReg          = VT3106J.reg, FET.reg, FlowCtrl.reg, FET.reg.win, AI.reg
CopyFiles       = FET.ndi.CopyFiles

[VT3106J.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg
AddReg          = VT3106J.reg, FET.reg, FlowCtrl.reg, FET.reg.NT, AI.reg
CopyFiles       = FET.CopyFiles.NT

[VT3106J.ndi.NT.Services]
AddService      = FETNDISB, 2, FET.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3065
;-------------------------------------------------------------------------------
[VT3065.ndi]
DelReg          = FET.delreg
AddReg          = VT3065.reg, FET.reg, FlowCtrl.reg, FET.reg.win, AI.reg
CopyFiles       = FET.ndi.CopyFiles

[VT3065.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg
AddReg          = VT3065.reg, FET.reg, FlowCtrl.reg, FET.reg.NT, AI.reg
CopyFiles       = FET.CopyFiles.NT

[VT3065.ndi.NT.Services]
AddService      = FETNDISB, 2, FET.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3043
;-------------------------------------------------------------------------------
[VT3043.ndi]
DelReg          = FET.delreg
AddReg          = VT3043.reg, FET.reg, FET.reg.win
CopyFiles       = FET.ndi.CopyFiles

[VT3043.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg
AddReg          = VT3043.reg, FET.reg, FET.reg.NT
CopyFiles       = FET.CopyFiles.NT

[VT3043.ndi.NT.Services]
AddService      = FETNDISB, 2, FET.Service, FET.EventLog

;-------------------------------------------------------------------------------
; VT3106S specific , AdapterCFID = 0x30531106 (HEX) = 810750214 (DEC)
;
[VT3106S.reg]
HKR, Ndi,                                   DeviceID,       0, "PCI\VEN_1106&DEV_3053"
HKR, ,                                      AdapterCFID,    0, "810750214"
HKR, ,                                      AdapterType,    0, "5"
HKR, ,                                      MediaType,      0, "1"

HKR, ,                                      ReceiveBurstIndicate,0,"64"
HKR, ,                                      ReceiveThreshold,   0, "0"
HKR, ,                                      TransmitThreshold,  0, "0"
HKR, ,                                      BurstLength,        0, "1"
HKR, ,                                      MapRegisters,       0, "32"
HKR, ,                                      EarlyReceive,       0, "0"
HKR, ,                                      EarlyTransmit,      0, "0"
; Nway Forced Mode
HKR, ,                                      NwayForce,          0, "1"
; Power Management Capability
HKR, ,                                      PMC,                0, "0"

HKR, ,                                      TransmitBuffers, 0, "64"
HKR, Ndi\params\TransmitBuffers,            ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers,            default,         0, "64"
HKR, Ndi\params\TransmitBuffers,            type,            0, "int"
HKR, Ndi\params\TransmitBuffers,            Min,             0, "48"
HKR, Ndi\params\TransmitBuffers,            Max,             0, "128"
HKR, Ndi\params\TransmitBuffers,            Step,            0, "1"
HKR, Ndi\params\TransmitBuffers,            Base,            0, "10"
HKR, Ndi\params\TransmitBuffers,            flag,            1, "20","00","00","00"

HKR, ,                                      ReceiveBuffers,  0, "64"
HKR, Ndi\params\ReceiveBuffers,             ParamDesc,       0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers,             default,         0, "64"
HKR, Ndi\params\ReceiveBuffers,             type,            0, "int"
HKR, Ndi\params\ReceiveBuffers,             Min,             0, "64"
HKR, Ndi\params\ReceiveBuffers,             Max,             0, "128"
HKR, Ndi\params\ReceiveBuffers,             Step,            0, "1"
HKR, Ndi\params\ReceiveBuffers,             Base,            0, "10"
HKR, Ndi\params\ReceiveBuffers,             flag,            1, "20","00","00","00"
;-------------------------------------------------------------------------------
; VT3106J specific , AdapterCFID = 0x31061106 (HEX) = 822481158 (DEC)
;
[VT3106J.reg]
HKR, Ndi,                                   DeviceID,       0, "PCI\VEN_1106&DEV_3106"
HKR, ,                                      AdapterCFID,    0, "822481158"
HKR, ,                                      AdapterType,    0, "5"
HKR, ,                                      MediaType,      0, "1"

HKR, ,                                      ReceiveBurstIndicate,0,"64"
HKR, ,                                      ReceiveThreshold,   0, "0"
HKR, ,                                      TransmitThreshold,  0, "0"
HKR, ,                                      BurstLength,        0, "1"
HKR, ,                                      MapRegisters,       0, "32"
HKR, ,                                      EarlyReceive,       0, "0"
HKR, ,                                      EarlyTransmit,      0, "0"
; Nway Forced Mode
HKR, ,                                      NwayForce,          0, "1"
; Power Management Capability
HKR, ,                                      PMC,                0, "0"

HKR, ,                                      TransmitBuffers, 0, "64"
HKR, Ndi\params\TransmitBuffers,            ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers,            default,         0, "64"
HKR, Ndi\params\TransmitBuffers,            type,            0, "int"
HKR, Ndi\params\TransmitBuffers,            Min,             0, "48"
HKR, Ndi\params\TransmitBuffers,            Max,             0, "128"
HKR, Ndi\params\TransmitBuffers,            Step,            0, "1"
HKR, Ndi\params\TransmitBuffers,            Base,            0, "10"
HKR, Ndi\params\TransmitBuffers,            flag,            1, "20","00","00","00"

HKR, ,                                      ReceiveBuffers,  0, "64"
HKR, Ndi\params\ReceiveBuffers,             ParamDesc,       0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers,             default,         0, "64"
HKR, Ndi\params\ReceiveBuffers,             type,            0, "int"
HKR, Ndi\params\ReceiveBuffers,             Min,             0, "64"
HKR, Ndi\params\ReceiveBuffers,             Max,             0, "128"
HKR, Ndi\params\ReceiveBuffers,             Step,            0, "1"
HKR, Ndi\params\ReceiveBuffers,             Base,            0, "10"
HKR, Ndi\params\ReceiveBuffers,             flag,            1, "20","00","00","00"
;-------------------------------------------------------------------------------
; VT3065 specific , AdapterCFID = 0x30651106 (HEX) = 811929862 (DEC)
;
[VT3065.reg]
HKR, Ndi,                                   DeviceID,       0, "PCI\VEN_1106&DEV_3065"
HKR, ,                                      AdapterCFID,    0, "811929862"
HKR, ,                                      AdapterType,    0, "5"
HKR, ,                                      MediaType,      0, "1"

HKR, ,                                      ReceiveBurstIndicate,0,"64"
HKR, ,                                      ReceiveThreshold,   0, "0"
HKR, ,                                      TransmitThreshold,  0, "0"
HKR, ,                                      BurstLength,        0, "1"
HKR, ,                                      MapRegisters,       0, "32"
HKR, ,                                      EarlyReceive,       0, "0"
HKR, ,                                      EarlyTransmit,      0, "0"
; Nway Forced Mode
HKR, ,                                      NwayForce,          0, "1"
; HW Phy Reset
HKR, ,                                      HWPhyReset,         0, "0"
; Power Management Capability
HKR, ,                                      PMC,                0, "0"

HKR, ,                                      TransmitBuffers, 0, "64"
HKR, Ndi\params\TransmitBuffers,            ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers,            default,         0, "64"
HKR, Ndi\params\TransmitBuffers,            type,            0, "int"
HKR, Ndi\params\TransmitBuffers,            Min,             0, "48"
HKR, Ndi\params\TransmitBuffers,            Max,             0, "128"
HKR, Ndi\params\TransmitBuffers,            Step,            0, "1"
HKR, Ndi\params\TransmitBuffers,            Base,            0, "10"
HKR, Ndi\params\TransmitBuffers,            flag,            1, "20","00","00","00"

HKR, ,                                      ReceiveBuffers,  0, "64"
HKR, Ndi\params\ReceiveBuffers,             ParamDesc,       0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers,             default,         0, "64"
HKR, Ndi\params\ReceiveBuffers,             type,            0, "int"
HKR, Ndi\params\ReceiveBuffers,             Min,             0, "64"
HKR, Ndi\params\ReceiveBuffers,             Max,             0, "128"
HKR, Ndi\params\ReceiveBuffers,             Step,            0, "1"
HKR, Ndi\params\ReceiveBuffers,             Base,            0, "10"
HKR, Ndi\params\ReceiveBuffers,             flag,            1, "20","00","00","00"
;-------------------------------------------------------------------------------
; VT3043 specific , AdapterCFID = 0x30431106 (HEX) = 809701638 (DEC)
;
[VT3043.reg]
HKR, Ndi,                                   DeviceID,       0, "PCI\VEN_1106&DEV_3043"
HKR, ,                                      AdapterCFID,    0, "809701638"
HKR, ,                                      AdapterType,    0, "5"
HKR, ,                                      MediaType,      0, "1"

HKR, ,                                      ReceiveBurstIndicate,0,"64"
HKR, ,                                      ReceiveThreshold,   0, "0"
HKR, ,                                      TransmitThreshold,  0, "0"
HKR, ,                                      BurstLength,        0, "1"
HKR, ,                                      MapRegisters,       0, "8"
HKR, ,                                      EarlyReceive,       0, "0"
HKR, ,                                      EarlyTransmit,      0, "0"

HKR, ,                                      TransmitBuffers, 0, "8"
HKR, Ndi\params\TransmitBuffers,            ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers,            default,         0, "8"
HKR, Ndi\params\TransmitBuffers,            type,            0, "int"
HKR, Ndi\params\TransmitBuffers,            Min,             0, "4"
HKR, Ndi\params\TransmitBuffers,            Max,             0, "64"
HKR, Ndi\params\TransmitBuffers,            Step,            0, "1"
HKR, Ndi\params\TransmitBuffers,            Base,            0, "10"
HKR, Ndi\params\TransmitBuffers,            flag,            1, "20","00","00","00"

HKR, ,                                      ReceiveBuffers,  0, "64"
HKR, Ndi\params\ReceiveBuffers,             ParamDesc,       0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers,             default,         0, "64"
HKR, Ndi\params\ReceiveBuffers,             type,            0, "int"
HKR, Ndi\params\ReceiveBuffers,             Min,             0, "64"
HKR, Ndi\params\ReceiveBuffers,             Max,             0, "128"
HKR, Ndi\params\ReceiveBuffers,             Step,            0, "1"
HKR, Ndi\params\ReceiveBuffers,             Base,            0, "10"
HKR, Ndi\params\ReceiveBuffers,             flag,            1, "20","00","00","00"
;-------------------------------------------------------------------------------
; FET common driver parameters
;
[FET.reg]

; Connection Type
HKR, ,                                      ConnectionType, 0, "0"
HKR, Ndi\params\ConnectionType,             ParamDesc,      0, %ConnectionType%
HKR, Ndi\params\ConnectionType,             default,        0, "0"
HKR, Ndi\params\ConnectionType,             type,           0, "enum"
HKR, Ndi\params\ConnectionType\enum,        0,              0, %autoN%
HKR, Ndi\params\ConnectionType\enum,        1,              0, %100HD%
HKR, Ndi\params\ConnectionType\enum,        2,              0, %100FD%
HKR, Ndi\params\ConnectionType\enum,        3,              0, %10HD%
HKR, Ndi\params\ConnectionType\enum,        4,              0, %10FD%
HKR, Ndi\params\ConnectionType,             flag,           1, "30","00","00","00"

; User defined Network Address
HKR, ,                                      NetworkAddress, 0, ""
HKR, Ndi\params\NetworkAddress,             ParamDesc,      0, %NetAddress%
HKR, Ndi\params\NetworkAddress,             Default,        0, ""
HKR, Ndi\params\NetworkAddress,             type,           0, "edit"
HKR, NDI\params\NetworkAddress,             LimitText,      0, "12"
HKR, NDI\params\NetworkAddress,             UpperCase,      0, "1"
HKR, NDI\params\NetworkAddress,             optional,       0, "1"
HKR, NDI\params\NetworkAddress,             Base,           0, "16"
HKR, Ndi\params\NetworkAddress,             flag,           1, "20","00","00","00"

; Validate Rx SNAP/802.3 packet length
HKR, ,                                      ValidatePacketLen, 0, "0"

[FlowCtrl.reg]
; Flow control capability advertisement
HKR, ,                                      FlowCtrl,        0, "0"
HKR, Ndi\params\FlowCtrl,                   ParamDesc,       0, %FlowCtl%
HKR, Ndi\params\FlowCtrl,                   default,         0, "0"
HKR, Ndi\params\FlowCtrl,                   type,            0, "enum"
HKR, Ndi\params\FlowCtrl\enum,              0,               0, %HwDefault%
HKR, Ndi\params\FlowCtrl\enum,              1,               0, %Disabled%
HKR, Ndi\params\FlowCtrl\enum,              2,               0, %Enabled%
HKR, Ndi\params\FlowCtrl,                   flag,            1, "20","00","00","00"

[FET.reg.win]
; Win95/Win98/Win
HKR, Ndi,                                   NdiInstaller,   0, "winndi.dll,NdiProc"
HKR, Ndi\Install,                           ndis3,          0, "FET.ndis5"

HKR, NDIS,                                  MajorNdisVersion,1,03
HKR, NDIS,                                  MinorNdisVersion,1,0A
HKR, ,                                      DevLoader,      0, "*ndis"
HKR, ,                                      DeviceVxDs,     0, "fetnd5a.sys"
HKR, NDIS,                                  LogDriverName,  0, "FETNDIS"
HKR, NDIS\NDIS2,                            DriverName,     0, "FETND$"
HKR, NDIS\NDIS2,                            FileName,       0, "fetnd.dos"
HKR, NDIS\ODI,                              DriverName,     0, "FETODI"
HKR, NDIS\ODI,                              FileName,       0, "fetodi.com"

HKR, Ndi\Interfaces,                        DefLower,       0, "ethernet"
HKR, Ndi\Interfaces,                        LowerRange,     0, "ethernet"
HKR, Ndi\Interfaces,                        DefUpper,       0, "ndis3,ndis2"
HKR, Ndi\Interfaces,                        UpperRange,     0, "ndis3"

; the parameter below are in windows 95(OSR2)/98(SE)/ME only
; Wake On LAN Event
HKR, ,                                      WOLEvent,        0, "0"
HKR, Ndi\params\WOLEvent,                   ParamDesc,       0, %WOLEvent%
HKR, Ndi\params\WOLEvent,                   default,         0, "0"
HKR, Ndi\params\WOLEvent,                   type,            0, "enum"
HKR, Ndi\params\WOLEvent\enum,              0,               0, %OSDefault%
HKR, Ndi\params\WOLEvent\enum,              1,               0, %OSAndUnicast%
HKR, Ndi\params\WOLEvent,                   flag,            1, "20","00","00","00"

[AI.reg]
; Adaptive Interrupt Capability
HKR, ,                                      AdaptiveInt,     0, "1"
HKR, Ndi\params\AdaptiveInt,                ParamDesc,       0, %AdaptiveInt%
HKR, Ndi\params\AdaptiveInt,                default,         0, "1"
HKR, Ndi\params\AdaptiveInt,                type,            0, "enum"
HKR, Ndi\params\AdaptiveInt\enum,           0,               0, %Disabled%
HKR, Ndi\params\AdaptiveInt\enum,           1,               0, %Enabled%
HKR, Ndi\params\AdaptiveInt,                flag,            1, "20","00","00","00"

[Tagging.reg]
; number of Tx queue allocation
HKR, ,                                      TxQueueNum,      0, "8"
; 802.1p/802.1q Packet Tagging
HKR, ,                                      8021pqtag,       0, "0"
HKR,Ndi\Params\8021pqtag,                   ParamDesc,       0, %8021pq%
HKR,Ndi\Params\8021pqtag,                   Default,         0, "0"
HKR,Ndi\Params\8021pqtag,                   type,            0, "enum"
HKR,Ndi\Params\8021pqtag\enum,              "0",             0, %Disabled%
HKR,Ndi\Params\8021pqtag\enum,              "1",             0, %Enabled%
HKR,Ndi\params\8021pqtag,                   flag,            1, "20","00","00","00"

[VLAN.reg]
; static single VLAN ID setting
HKR, ,                                      VLANID,          0, "0"
HKR, Ndi\params\VLANID,                     ParamDesc,       0, %VLANID%
HKR, Ndi\params\VLANID,                     default,         0, "0"
HKR, Ndi\params\VLANID,                     type,            0, "int"
HKR, Ndi\params\VLANID,                     Min,             0, "0"
HKR, Ndi\params\VLANID,                     Max,             0, "4094"
HKR, Ndi\params\VLANID,                     Step,            0, "1"
HKR, Ndi\params\VLANID,                     Base,            0, "10"
HKR, Ndi\params\VLANID,                     flag,            1, "20","00","00","00"

[FET.reg.NT]
; Windows 2000/XP
HKR, Ndi\Interfaces,                        LowerRange,      0, "ethernet"
HKR, Ndi\Interfaces,                        UpperRange,      0, "ndis5"
HKR, Ndi,                                   Service,         0, "FETNDISB"

; Win2K ScatterGather DMA Capability
HKR, ,                                      2KScatterGather, 0, "0"


[Cksumoffload.reg.NT]
HKR, ,                                      Checksum,        0, "0"
HKR, Ndi\params\Checksum,                   ParamDesc,       0, %checksum%
HKR, Ndi\params\Checksum,                   default,         0, "0"
HKR, Ndi\params\Checksum,                   type,            0, "enum"
HKR, Ndi\params\Checksum\enum,              0,               0, %Disabled%
HKR, Ndi\params\Checksum\enum,              1,               0, %Enabled%
HKR, Ndi\params\Checksum,                   flag,            1, "20","00","00","00"

;-------------------------------------------------------------------------------
; Installation for NT
;

[FET.CopyFiles.NT]
fetnd5b.sys,,,2

[FET.Service]
DisplayName     = %FET.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\fetnd5b.sys
LoadOrderGroup  = NDIS

[FET.EventLog]
AddReg = FET.AddEventLog.reg

[FET.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; Installation for Windows 95/98/ME
;

[FET.ndis5]
CopyFiles=FET.ndis5.CopyFiles

[FET.ndis4]
CopyFiles=FET.ndis4.CopyFiles

[FET.ndis3]
CopyFiles=FET.ndis3.CopyFiles

[FET.ndis2]
CopyFiles=FET.ndis2.CopyFiles

[FET.odi]
CopyFiles=FET.odi.CopyFiles

;-------------------------------------------------------------------------------
; CopyFiles sections for Windows 95/98/ME
;

[FET.ndi.CopyFiles]
winndi.dll,,,2

[FET.ndis5.CopyFiles]
fetnd5a.sys,,,2

[FET.ndis4.CopyFiles]
fetnd4.sys,,,2

[FET.ndis3.CopyFiles]
fetnd3.sys,,,2

[FET.ndis2.CopyFiles]
fetnd.dos

[FET.odi.CopyFiles]
fetodi.com

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir          = 11
FET.CopyFiles.NT        = 12
FET.ndis2.CopyFiles     = 10
FET.odi.CopyFiles       = 10

[SourceDisksFiles]
fetnd5a.sys         = 1
fetnd5b.sys         = 1
fetnd4.sys          = 1
fetnd3.sys          = 1
fetndis.inf         = 1
winndi.dll          = 1
fetnd.dos           = 1
fetodi.com          = 1

[SourceDisksNames]
1 = %DiskName%,,,

;-------------------------------------------------------------------------------
; Uninstall/DelFiles/DelReg
;
[FET.delreg]
HKR,Ndi\Params

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Prov                = "VIA"
DiskName            = "Network Adapter source disk"
ConnectionType      = "Connection Type"
autoN               = "Auto-Negotiation"
100HD               = "100BaseTx Half Duplex"
100FD               = "100BaseTx Full Duplex"
10HD                = "10BaseT   Half Duplex"
10FD                = "10BaseT   Full Duplex"
Disabled            = "Disabled"
Enabled             = "Enabled"
WOLEvent            = "Wake On LAN Event"
OSDefault           = "OS Default Event"
OSAndUnicast        = "OS Default & Unicast"
TXBuffer            = "Transmit Buffers"
RXBuffer            = "Receive Buffers"
NetAddress          = "Network Address"
FlowCtl             = "Flow Control"
HwDefault           = "Hardware Default"
8021pq              = "802.1p/Q Tagging"
VLANID              = "VLAN ID"
AdaptiveInt         = "Adaptive Interrupt"
checksum            = "Checksum Offload"

Manuf   = "VIA Technologies, Inc."
VT3106S.DeviceDesc   = "VIA Rhine III Management Adapter"
VT3106J.DeviceDesc   = "VIA Rhine III Fast Ethernet Adapter"
VT3065.DeviceDesc    = "VIA Rhine II Fast Ethernet Adapter"
VT3043.DeviceDesc    = "VIA VT86C100A Rhine Fast Ethernet Adapter"
FET.Service.DispName = "VIA Rhine Family Fast Ethernet Adapter Driver Service"
