;DrIvEr DeScRiPtIoN
;VeRsIoN = 3.03 Novell LAN Installation Information File for FETNWSA
;CoPyRiGhT = (c) Copyright 2001 by VIA. All rights reserved.

VER: 3.03                                       ; This LDI version
SYN: 1.00

; ----------------------------------
;           VT3053 
; ----------------------------------
DR VT_3053
{
        DES:    $VT_DES_3053
        HELP:   $VT_HELP
        PAR:    2.00                            ; Hardware Instance Number Aware
        PROD:   'PCI.1106.3053.*.*.*'           ; VT3053
                
        FILE:   FETNWSA.LAN
        
        ;@#	CLIENT:	FETNWSA.LAN
        ;@#	ALIAS:	FETNWSA.LAN
        ;@# SPROD:  'VIA~ VIA Rhine III Management Adapter'

        PROMPT SLOT OPTIONAL
        {
                DES:    $VT_SLOT_DES
                HELP:   $VT_SLOT_HLP

                TYPE:   DECIMAL(5)
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'SLOT=%s'
        }

        PR NODE
        {
        }

        FR FrameSelect
        {
                CH:     'Ethernet_802.3'
                CH:     'Ethernet_802.2'
                CH:     'Ethernet_SNAP'
                CH:     'Ethernet_II'
                DEF:    1,2                 ; Default flame type = 802.3, 802.2
        }

        ; ---------------------------------------------------------
        ; LIST keywords [CONNECTIONTYPE]:
        ;   AUTOSENSE, 10BASET, 10BASETFD, 100BASETX, 100BASETXFD     
        ; ---------------------------------------------------------
        LI CONNECTIONTYPE OPT
        {
                DES:    $VT_CONTYPE_DES
                HELP:   $VT_CONTYPE_HLP

                CD:     $VT_CAUTO_CD
                CH:     $VT_CAUTO_CH
                CD:     $VT_C10H_CD
                CH:     $VT_C10H_CH
                CD:     $VT_C10F_CD
                CH:     $VT_C10F_CH
                CD:     $VT_C100H_CD
                CH:     $VT_C100H_CH
                CD:     $VT_C100F_CD
                CH:     $VT_C100F_CH
                DEF:    1                       ; DEFAULT=AUTOSENSE
                
                OUT:    'CONNECTIONTYPE=%s'     ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'CONNECTIONTYPE'
        }
        
        ; ---------------------------------------------------------
        ; keywords [VID]:
        ;   0 ~ 4096
        ; ---------------------------------------------------------
        PROMPT VID OPTIONAL
        {
                DES:    $VT_VID_DES
                HELP:   $VT_VID_HLP

                TYPE:   DECIMAL(4)
                VAL:    1-4094
                DEF:    UNDEFINED
                OUT:    'VID=%s'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [FLOW_CONTROL]:
        ;   Enable, Disable, Hardware_default(or HD)
        ; --------------------------------------------------
        LI FLOW_CONTROL OPT
        {
                DES:    $VT_FLOWCTL_DES
                HELP:   $VT_FLOWCTL_HLP

                CD:     $VT_FHD_CD
                CH:     $VT_FHD_CH
                CD:     $VT_FENA_CD
                CH:     $VT_FENA_CH
                CD:     $VT_FDIS_CD
                CH:     $VT_FDIS_CH
                DEF:    1                       ; DEFAULT=Hardware_Default (HD)
                
                OUT:    'FLOW_CONTROL=%s'       ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'FLOW_CONTROL'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [TAG]:
        ;   Enable, Disable
        ; --------------------------------------------------
        LI TAG OPT
        {
                DES:    $VT_TAG_DES
                HELP:   $VT_TAG_HLP

                CD:     $VT_TENA_CD
                CH:     $VT_TENA_CH
                CD:     $VT_TDIS_CD
                CH:     $VT_TDIS_CH
                DEF:    2                       ; DEFAULT=Disable
                OUT:    'TAG=%s'                ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'TAG'
                                                
                ;DES:    $VT_PRI_DES
                ;HELP:   $VT_PRI_HLP

                ;CD:     $VT_PENA_CD
                ;CH:     $VT_PENA_CH
                ;CD:     $VT_PDIS_CD
                ;CH:     $VT_PDIS_CH
                ;DEF:    2                       ; DEFAULT=Disable
                ;OUT:    'PRIORITY=%s'           ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'PRIORITY'
        }
        
}

; ----------------------------------
;           VT3106 
; ----------------------------------
DR VT_3106
{
        DES:    $VT_DES_3106
        HELP:   $VT_HELP
        PAR:    2.00                            ; Hardware Instance Number Aware
        PROD:   'PCI.1106.3106.*.*.*'           ; VT3106
                
        FILE:   FETNWSA.LAN
        
        ;@#	CLIENT:	FETNWSA.LAN
        ;@#	ALIAS:	FETNWSA.LAN
        ;@# SPROD:  'VIA~ VIA Rhine III Fast Ethernet Adapter'

        PROMPT SLOT OPTIONAL
        {
                DES:    $VT_SLOT_DES
                HELP:   $VT_SLOT_HLP

                TYPE:   DECIMAL(5)
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'SLOT=%s'
        }

        PR NODE
        {
        }

        FR FrameSelect
        {
                CH:     'Ethernet_802.3'
                CH:     'Ethernet_802.2'
                CH:     'Ethernet_SNAP'
                CH:     'Ethernet_II'
                DEF:    1,2                 ; Default flame type = 802.3, 802.2
        }

        ; ---------------------------------------------------------
        ; LIST keywords [CONNECTIONTYPE]:
        ;   AUTOSENSE, 10BASET, 10BASETFD, 100BASETX, 100BASETXFD     
        ; ---------------------------------------------------------
        LI CONNECTIONTYPE OPT
        {
                DES:    $VT_CONTYPE_DES
                HELP:   $VT_CONTYPE_HLP

                CD:     $VT_CAUTO_CD
                CH:     $VT_CAUTO_CH
                CD:     $VT_C10H_CD
                CH:     $VT_C10H_CH
                CD:     $VT_C10F_CD
                CH:     $VT_C10F_CH
                CD:     $VT_C100H_CD
                CH:     $VT_C100H_CH
                CD:     $VT_C100F_CD
                CH:     $VT_C100F_CH
                DEF:    1                       ; DEFAULT=AUTOSENSE
                
                OUT:    'CONNECTIONTYPE=%s'     ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'CONNECTIONTYPE'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [FLOW_CONTROL]:
        ;   Enable, Disable, Hardware_default(or HD)
        ; --------------------------------------------------
        LI FLOW_CONTROL OPT
        {
                DES:    $VT_FLOWCTL_DES
                HELP:   $VT_FLOWCTL_HLP

                CD:     $VT_FHD_CD
                CH:     $VT_FHD_CH
                CD:     $VT_FENA_CD
                CH:     $VT_FENA_CH
                CD:     $VT_FDIS_CD
                CH:     $VT_FDIS_CH
                DEF:    1                       ; DEFAULT=Hardware_Default (HD)
                
                OUT:    'FLOW_CONTROL=%s'       ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'FLOW_CONTROL'
        }
}

; ----------------------------------
;           VT3065 
; ----------------------------------
DR VT_3065
{
        DES:    $VT_DES_3065
        HELP:   $VT_HELP
        PAR:    2.00                            ; Hardware Instance Number Aware
        PROD:   'PCI.1106.3065.*.*.*'           ; VT3065
                
        FILE:   FETNWSA.LAN
        
        ;@#	CLIENT:	FETNWSA.LAN
        ;@#	ALIAS:	FETNWSA.LAN
        ;@# SPROD:  'VIA~ VIA Rhine II Fast Ethernet Adapter'

        PROMPT SLOT OPTIONAL
        {
                DES:    $VT_SLOT_DES
                HELP:   $VT_SLOT_HLP

                TYPE:   DECIMAL(5)
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'SLOT=%s'
        }

        PR NODE
        {
        }

        FR FrameSelect
        {
                CH:     'Ethernet_802.3'
                CH:     'Ethernet_802.2'
                CH:     'Ethernet_SNAP'
                CH:     'Ethernet_II'
                DEF:    1,2                 ; Default flame type = 802.3, 802.2
        }

        ; ---------------------------------------------------------
        ; LIST keywords [CONNECTIONTYPE]:
        ;   AUTOSENSE, 10BASET, 10BASETFD, 100BASETX, 100BASETXFD     
        ; ---------------------------------------------------------
        LI CONNECTIONTYPE OPT
        {
                DES:    $VT_CONTYPE_DES
                HELP:   $VT_CONTYPE_HLP

                CD:     $VT_CAUTO_CD
                CH:     $VT_CAUTO_CH
                CD:     $VT_C10H_CD
                CH:     $VT_C10H_CH
                CD:     $VT_C10F_CD
                CH:     $VT_C10F_CH
                CD:     $VT_C100H_CD
                CH:     $VT_C100H_CH
                CD:     $VT_C100F_CD
                CH:     $VT_C100F_CH
                DEF:    1                       ; DEFAULT=AUTOSENSE
                
                OUT:    'CONNECTIONTYPE=%s'     ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'CONNECTIONTYPE'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [FLOW_CONTROL]:
        ;   Enable, Disable, Hardware_default(or HD)
        ; --------------------------------------------------
        LI FLOW_CONTROL OPT
        {
                DES:    $VT_FLOWCTL_DES
                HELP:   $VT_FLOWCTL_HLP

                CD:     $VT_FHD_CD
                CH:     $VT_FHD_CH
                CD:     $VT_FENA_CD
                CH:     $VT_FENA_CH
                CD:     $VT_FDIS_CD
                CH:     $VT_FDIS_CH
                DEF:    1                       ; DEFAULT=Hardware_Default (HD)
                
                OUT:    'FLOW_CONTROL=%s'       ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'FLOW_CONTROL'
        }
}

; ----------------------------------
;           VT3043 
; ----------------------------------
DR VT_3043
{
        DES:    $VT_DES_3043
        HELP:   $VT_HELP
        PAR:    2.00                            ; Hardware Instance Number Aware
        PROD:   'PCI.1106.3043.*.*.*'           ; VT3043
                
        FILE:   FETNWSA.LAN
        
        ;@#	CLIENT:	FETNWSA.LAN
        ;@#	ALIAS:	FETNWSA.LAN
        ;@# SPROD:  'VIA~ VIA VT86C100A Rhine Fast Ethernet Adapter'

        PROMPT SLOT OPTIONAL
        {
                DES:    $VT_SLOT_DES
                HELP:   $VT_SLOT_HLP

                TYPE:   DECIMAL(5)
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'SLOT=%s'
        }

        PR NODE
        {
        }

        FR FrameSelect
        {
                CH:     'Ethernet_802.3'
                CH:     'Ethernet_802.2'
                CH:     'Ethernet_SNAP'
                CH:     'Ethernet_II'
                DEF:    1,2                 ; Default flame type = 802.3, 802.2
        }

        ; ---------------------------------------------------------
        ; LIST keywords [CONNECTIONTYPE]:
        ;   AUTOSENSE, 10BASET, 10BASETFD, 100BASETX, 100BASETXFD     
        ; ---------------------------------------------------------
        LI CONNECTIONTYPE OPT
        {
                DES:    $VT_CONTYPE_DES
                HELP:   $VT_CONTYPE_HLP

                CD:     $VT_CAUTO_CD
                CH:     $VT_CAUTO_CH
                CD:     $VT_C10H_CD
                CH:     $VT_C10H_CH
                CD:     $VT_C10F_CD
                CH:     $VT_C10F_CH
                CD:     $VT_C100H_CD
                CH:     $VT_C100H_CH
                CD:     $VT_C100F_CD
                CH:     $VT_C100F_CH
                DEF:    1                       ; DEFAULT=AUTOSENSE
                
                OUT:    'CONNECTIONTYPE=%s'     ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'CONNECTIONTYPE'
        }
}


DLANG:  4
;English
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"
                                        
        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   6
;French
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"
                                        
        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"

        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."
LANG:   7
;German
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   8
;Italian
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   14
;Spanish
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   9
;Japanese
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   10
;Korean
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."

        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                       
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   12
;Portugese (Brazil)
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   13
;Russian
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   16
;Chinese (Traditional)
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   1
;Chinese (Simplified)
        $VT_DUPLEX_DES= "Full Duplex mode"
        $VT_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $VT_AUTO_DES  = "AUTO mode"
        $VT_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $VT_SPEED_DES = "SPEED selection"
        $VT_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $VT_SLOT_DES  = "Slot"
        $VT_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $VT_CONTYPE_DES   = "Media and Line Speed"
        $VT_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_PRI_DES   = "Priority Transmit Support"
        $VT_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $VT_TAG_DES   = "Tagging ability Support"
        $VT_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $VT_FLOWCTL_DES   = "Flow control ability"
        $VT_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $VT_HCS_DES   = "Hardware Checksum Support"
        $VT_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $VT_VID_DES   = "VID number support for VLAN"
        $VT_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $VT_CAUTO_CD  = "Auto-Sense media type"
        $VT_CAUTO_CH  = "Autosense"
        $VT_C10H_CD   = "Twisted Pair 10MBPS"
        $VT_C10H_CH   = "10BASET"
        $VT_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $VT_C10F_CH   = "10BASETFD"
        $VT_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $VT_C100H_CH  = "100BASETXFD"
        $VT_C100F_CD  = "Fast Ethernet 100MBPS"
        $VT_C100F_CH  = "100BASETX"
        

        $VT_FHD_CD    = "Use Hardware Default"
        $VT_FHD_CH    = "Hardware_Default"
        $VT_FENA_CD   = "Enable Flow Control"
        $VT_FENA_CH   = "Enable"
        $VT_FDIS_CD   = "Disable Flow Control"
        $VT_FDIS_CH   = "Disable"
        
        
        $VT_PENA_CD   = "Enable Priority Transmit"
        $VT_PENA_CH   = "Enable"
        $VT_PDIS_CD   = "Disable Priority Transmit"
        $VT_PDIS_CH   = "Disable"
                                        
        $VT_TENA_CD   = "Enable Tagging"
        $VT_TENA_CH   = "Enable"
        $VT_TDIS_CD   = "Disable Tagging"
        $VT_TDIS_CH   = "Disable"
        
        $VT_HENA_CD   = "Enable Hardware Checksum"
        $VT_HENA_CH   = "Enable"
        $VT_HDIS_CD   = "Disable Hardware Checksum"
        $VT_HDIS_CH   = "Disable"

        $VT_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $VT_DES_3053  = "VIA Rhine III Management Adapter"
        $VT_DES_3106  = "VIA Rhine III Fast Ethernet Adapter"
        $VT_DES_3065  = "VIA Rhine II Fast Ethernet Adapter"
        $VT_DES_3043  = "VIA VT86C100A Rhine Fast Ethernet Adapter"
        $VT_HELP      = "This driver (FETNWSA.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

;DrIvEr DeScRiPtIoN EnD
