 
# IMPORTANT INFO!
 
- Most of 100/200 boards should work fine with 12-thread CPUs after 12T_blocker fix applied even on
  latest 3xxx bioses. But if it won't, use hint described below to bypass issue.
 
- If system won't work with this bios after modification then try to modify earlier version of bios 
  (under 3000 for 100-series and under 1000 for 200-series).
 
 
# NOTE FOR XEON ONLY!
 
- This bios may cause ONE_BOOT_BUG issue: first boot into system will success, but after reboot it
  won't boot even in bios. Detaching HDD will allow you to enter in bios, but still not in OS.
 
- This bug found only for Coffee Xeon CPUs and can't be fixed yet.
 
- Try to use earlier 2xxx bios version to bypass this bug.
 