!
!     # ABOUT COFFEE REVISIONS
!
!     B0 - Has "old" textolite, same as skylake/kabylake CPUs, and assigned with 906EB mCode.
!          It's easy for mod bios and not needed any shorting/isolating work. Almost all of 
!          i3/Pentium/Celeron use it.
!
!     U0 - Has "new" textolite with a bit other pinout, needs 906EA mCode. Requires SKU hack
!          mod and shorting/isolating some pins, board vendor depends. All 8th Gen i5 and i7
!          has this one.
!
!     P0 - CFL Refresh textolite. Visually a bit other than U0. Used by all 9th Gen CPUs, needs
!          906EC mCode. Requires the same mod list as U0 (same dependencies by threads count).
!
!     According official info i3 8100, G5400 and G5400T can use B0 and U0 revisions, but all
!     known i3 8100 has B0 revision and Pentium G5400/G5400T - U0. There are no noticed incidents
!     with i3 8100-U0, G5400-B0 or G5400T-B0 at the moment. So we can expect that i3 8100 will
!     require B0-mod and G5400/G5400T - U0-mod. Anyway CoffeeTime can make both.
!
!     CPU revision can be identified by visual. Check out comparison image.
!