Warning: By flashing your motherboard, you agree to accept the possibility of BIOS flash failure.
If your System is stable and working we recommend that you DO NOT try to upgrade your BIOS.


To flash bios, please create a bootable floopy disk and copy awdf815b.exe and your 
*.bin (e.g. r01f3.bin) file to it. 

At the dos prompt type in: 

awdf815b  *****.bin /sn/py/cd/cp/qi/cksee1c/r

for example: awdf815b  r01f3.bin /sn/py/cd/cp/qi/cksee1c/r

---------------------

Um das Bios Ihres Rechners zu flashen, legen Sie sich bitte eine bootfähige Diskette an, kopieren die Dateien flash810.exe und die *.bin (z.B. r01f3.bin) auf diese.
Am Dos-Prompt geben Sie bitte ein: 

awdf815b  *****.bin /sn/py/cd/cp/qi/cksee1c/r

z.B. awdf815b  r01f3.bin /sn/py/cd/cp/qi/cksee1c/r
 